**Plastic Sheet Lines**

**PC Plastic Sheet Line**

It is used to produce PC transparent sheet and PC functional sheet, for auto industry, electronic industry, electrical equipment industry, face shield, safety helmet and etc.

Width: 800-1250mm; thickness: 0.15-1mm; capacity: 400-600kg/hr

**Multi-layer Co-extrusion Plastic Sheet Line**

It is used to produce compound functional sheet, such as five or seven layer PP barrier sheet for food fresh packaging; three layer PS conductive sheet for electronic packaging; four layer PS sheet for yogurt packaging.

**PET Plastic Sheet Line**

It is used to produce APET/PETG plastic sheet, mono-layer, two-layer or three-layer compound sheet. There is single screw and twin screw sheet line.

Width: 600-1300mm; thickness: 0.12-2mm; capacity: 300-1000kg/hr

**Online One-step Solar Back Film Line**

Changed the previous mode of production，Shorten and simplify the production process，the base and laminated film one step. And it saves space, is environmental protection, high efficient, low cost.

**Polyolefin Plastic Board Line**

It is used to produce polyolefin board, such as PE, PP, PS, ABS and etc.

Width: 1000-2200mm; thickness: 1-15mm

